

**Packet Tracer - Basic Device Configuration**

**Topology**

You will receive one of three possible topologies.

# Addressing Table

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Device** | **Interface** |  | **IP Address** | **Default Gateway** |
| *blank*    RTA | G0/0  *G0/0*  *G0/0* |  | 10.10.10.1/24 | N/A  *N/A*  *N/A* |
|  | 2001:DB8:ACAD:100::1/64 |
|  | FE80::1 |
| G0/1  *G0/1*  *G0/1* |  | 10.10.11.1/24 | N/A  *N/A*  *N/A* |
|  | 2001:DB8:ACAD:200::1/64 |
|  | FE80::1 |
| ASw-1 | VLAN 1 |  |  | 10.10.10.1 |
| ASw-2 | VLAN 1 |  | 10.10.11.2/24 | 10.10.11.1 |
| User-01 | NIC  *NIC* |  | 10.10.10.101/24 | 10.10.10.1 |
|  | 2001:DB8:ACAD:100::2/64 | FE80::1 |
| *User-02* | NIC  *NIC* |  | 10.10.10.102/24 | 10.10.10.1 |
|  | 2001:DB8:ACAD:100::3/64 | FE80::1 |
| *User-03* | NIC  *NIC* |  | 10.10.11.101/24 | 10.10.11.1 |
|  | 2001:DB8:ACAD:200::2/64 | FE80::1 |
| *User-04* | NIC  *NIC* |  | 10.10.11.102/24 | 10.10.11.1 |
|  | 2001:DB8:ACAD:200::3/64 | FE80::1 |

# Objectives

* Complete the network documentation.
* Perform basic device configurations on a router and a switch.
* Verify connectivity and troubleshoot any issues.

# Scenario

Your network manager is impressed with your performance in your job as a LAN technician. She would like you to demonstrate your ability to configure a router that connects two LANs. Your tasks include configuring basic settings on a router and a switch using the Cisco IOS. You will also configure IPv6 addresses on network devices and hosts. You will then verify the configurations by testing end-to-end connectivity. You goal is to establish connectivity between all devices.

© 2013 - 2019 Cisco and/or its affiliates. All rights reserved. Cisco Public Page **1** of **2** www.netacad.com

## Packet Tracer - Basic Device Configuration

**Note:** The VLAN1 interface on  will not be reachable over IPv6.

In this activity you will configure the  router,  switch, and the **PC hosts**.

**Note:** Packet Tracer will not score some configured values, however these values are required to accomplish full connectivity in the network.

# Requirements

* Provide the missing information in the Addressing Table.
* Name the router and the second switch . You will not be able to access the switch.
* Use **cisco** as the user EXEC password for all lines.
* Use **class** as the encrypted privileged EXEC password.
* Encrypt all plaintext passwords.
* Configure an appropriate banner.
* Configure IPv4 and IPv6 addressing for the  switch according to the Addressing Table.
* Configure IPv4 and IPv6 addressing for the  switch according to the Addressing Table.
* The hosts are partially configured. Complete the IPv4 addressing, and fully configure the IPv6 addresses according to the Addressing Table.
* Document interfaces with descriptions, including the  VLAN 1 interface.
* Save your configurations.
* Verify connectivity between all devices. All devices should be able to ping all other devices with IPv4 and IPv6.
* Troubleshoot and document any issues.
* Implement the solutions necessary to enable and verify full end-to-end connectivity.

**Note**: Click **Check Results** button to see your progress. Click the **Reset Activity** button to generate a new set of requirements.

*End of document*

© 2013 - 2019 Cisco and/or its affiliates. All rights reserved. Cisco Public Page **2** of **2** www.netacad.com